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Сажетак: Пестициди представљају значајне загађиваче водених екосистема, због чега је развој одрживих материјала за њихово уклањање предмет бројних истраживања. Пивски троп, као главни нуспроизвод пиварске индустрије, представља лигноцелулозну биомасу са израженим адсорпционим потенцијалом који произилази из њене порозне структуре и присуства различитих функционалних група. У овом раду разматран је потенцијал пивског тропа као биоадсорбента за уклањање одабраних пестицида из водених раствора, уз осврт на његове структурне карактеристике, адсорпциони капацитет и факторе који утичу на ефикасност процеса. Посебна пажња посвећена је значају пивског тропа у контексту зелене хемије, циркуларне економије и валоризације отпада. Досадашња истраживања указују да је пивски троп еколошки прихватљив, обновљив и економичан адсорбент са великим потенцијалом за пречишћавање вода.
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BREWER'S SPENT GRAIN AS A SUSTAINABLE BIO-BASED ADSORBENT FOR THE REMOVAL OF SELECTED PESTICIDES FROM AQUEOUS MEDIA

Abstract: Pesticides are significant pollutants of aquatic ecosystems, prompting extensive research into the development of sustainable materials for their removal. Brewer’s spent grain, the main by-product of the brewing industry, represents a lignocellulosic biomass with considerable adsorption potential arising from its porous structure and the presence of various functional groups. This paper discusses the potential of brewer’s spent grain as a bioadsorbent for the removal of selected pesticides from aqueous solutions, with emphasis on its structural characteristics, adsorption capacity, and factors influencing process efficiency. The importance of brewer’s spent grain in the context of green chemistry, circular economy, and waste valorization is also considered. Previous studies indicate that brewer’s spent grain is an environmentally friendly, renewable, and cost-effective adsorbent with significant potential for water purification.
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